In a hydraulic jack a small and a large fluid-filled cylinder are joined together by a pipe. The pump is powered by gearwheels that push fluid into the hydraulic piston to raise weights.