In the enormous electromagnets, located on both sides of the guideway in the magnetic levitation railway, the strength of current flowing through it is automatically regulated so that the train is always held in the right position.