In liquid fuel rockets, liquid propellant (e.g. hydrogen) and oxidizer (pure oxygen) are fed together into a combustion chamber. Unlike solid fuel rockets, liquid fuel burners can be reduced, switched on or off.