Apple II
Technical Notes
_____________________________________________________________________________
                                                  Developer Technical Support

Apple IIGS
#36:    Port Driver Specifications

Revised by:    Matt Deatherage & Suki Lee                        January 1989
Written by:    Dan Hitchens                                          May 1988

This Technical Note describes how to write your own drivers for Apple IIGS 
ports.
Changed since November 1988:  Corrects errors in the descriptions of 
PrDevRead and PrDevAsyncRead.
_____________________________________________________________________________


Introduction

A port driver handles certain hardware-specific duties for the Print Manager, 
such as initializing firmware and handling low-level hardware handshaking 
protocols, if any are implemented.  The port driver structure, like the 
printer driver structure, insulates the Print Manager from low-level details 
of printers and interface cards (or ports) so that the same calls work across 
various hardware configurations, provided drivers are installed on the boot 
disk.

Note that a port driver could also easily be called a "card driver;" the term 
"port" is used because the first ones written were for the internal ports of 
the Apple IIGS.  A port driver could interface any printer (for which there is 
a printer driver) with any kind of port or peripheral card that can handle it.  
A familiar example would be a parallel printer interface card - a port driver 
for a parallel card would enable the Print Manager to print graphics to any 
parallel printer connected to it (provided, again, there was a printer driver 
for the particular printer installed).

In general, you need a port driver for each port or interface card through 
which you intend to print, and a printer driver for each printer to which you 
intend to print.  On System Disk 4.0, Apple provides port driver files for the 
printer port (PRINTER), the modem port (MODEM), a port connected to the 
AppleTalk network (APPLETALK), and a parallel printer interface card 
(PARALLEL.CARD).  Apple also provides printer drivers for the ImageWriter and 
ImageWriter II (IMAGEWRITER), the ImageWriter LQ (IMAGEWRITER.LQ), the 
LaserWriter family.(LASERWRITER), and an Epson (EPSON).  With this 
configuration, you can print to any of the printer types above through any of 
the ports, cards, or over AppleTalk.  Other printer drivers and port drivers 
would extend the user's selection of available configurations.


What's in a Port Driver

File Structure

Users can install new port drivers into the system by copying a port driver 
file into a subdirectory called DRIVERS within the SYSTEM subdirectory or by 
running the Installer if the driver is supplied with a script to install it.  
The port driver file must be of type $BB.  There are two kinds of port 
drivers:  local drivers, intended to drive a printer connected locally, and 
network drivers, which handle printers connected over an AppleTalk network.  
Local drivers have an auxiliary type of $0002, and AppleTalk drivers (there 
should be only one) have an auxiliary type of $0003.

Port Driver Calls

A port driver must support the following calls:

    PrDevPrChanged          $1913
    PrDevStartup            $1A13
    PrDevShutDown           $1B13
    PrDevOpen               $1C13
    PrDevRead               $1D13
    PrDevWrite              $1E13
    PrDevClose              $1F13
    PrDevStatus             $2013
    PrDevAsyncRead          $2113    (alias PrDevInitBack)
    PrDevWriteBackground    $2213    (alias PrDevFillBack)
    PrPortVer               $2413
    PrDevIsItSafe           $3013

Note that a network port driver has much more work to do than a regular 
(local) port or card driver.  A local driver only has to worry about one 
printer, whereas a network port driver may find that there is not even a 
printer available on a running network.  The information on network drivers is 
provided mostly for informational purposes; you should never find it necessary 
to write your own AppleTalk port driver.

Entering and Exiting a Port Driver 

Entering and exiting is the same as described for the printer driver calls in 
Apple IIGS Technical Note #35, "Printer Driver Specifications."



PrDevPrChanged           $1913

Description:
    The Print Manager makes this call every time the user accepts this port 
    driver in the Choose Printer dialog.

Input:                   LONG        printer name pointer

Direct Connect:
o   Makes sure that this port has been set up correctly in the Control Panel 
    (parity, baud rate, etc.), and puts up an alert for the user if it has not 
    been.  Remember that if you change settings, even at the user's request, 
    you should change the Battery RAM parameters as well, so the setting 
    changes will be reflected when the user enters the Control Panel.

Network:
o   Copies the printer name to local storage for use in the NBPLookup function 
    of the AppleTalk PAPopen and PAPstatus calls, usually by placing it in the 
    AppleTalk parameter block.  This function is similar to that performed by 
    PrStartUp, except that PrDevPrChanged is called whenever the printer is 
    changed by the user with the Choose Printer dialog.


PrDevStartUp             $1A13

Description:
    This call is not required to do anything.  However, if your driver needs to 
    initialize itself by allocating memory or other setup tasks, this is the 
    place to do it.  Network drivers should copy the printer name to a local 
    storage area for later use.

Input:                   LONG        printer name pointer
                         LONG        zone name pointer

Direct Connect:
o   Required to do nothing.  This is a good place to do your own set-up tasks, 
    if you have any.

Network:
o   Copies the printer name and the zone name to local storage for use in the 
    NBPLookup function of the AppleTalk PAPopen and PAPstatus calls, usually by 
    placing it in the AppleTalk parameter block.


PrDevShutDown            $1B13

Description:
    This call, like PrDevStartUp, is not required to do anything.  However, if 
    your driver performs other tasks when it starts, from the normal 
    (allocating memory) to the obscure (installing heartbeat tasks), it should 
    undo them here.  If you allocate anything when you start, you should 
    deallocate it when you shutdown.  Note that this call may be made without a 
    balancing PrDevStartUp, so be prepared for this instance.  For example, do 
    not try to blindly deallocate a handle that your PrDevStartUp routine 
    allocates and stores in local storage; if you have not called PrDevStartUp, 
    there is no telling what will be in your local storage area.

Input:                   none

PrDevOpen                $1C13

Description:
    This call basically prepares the firmware for printing.  It must initialize 
    the firmware for both input and output.  Input is required so the connected 
    printer may be polled for its status.

    A network driver has considerably more work to do, including the 
    possibility of asynchronous communications.  Details are provided below.

Input:                   LONG        completion routine pointer 
                         LONG        reserved long

Direct Connect:
o   Initializes the firmware for input and output, preparing for reading from 
    or writing to the printer.
o   If the completion pointer is NIL, then RTL.  If it is not NIL, then perform 
    a JSL to the completion routine.

Network:
o   Initializes the End-Of-Write parameter in the AppleTalk PAPWrite parameter 
    block to zero.  Never call AppleTalk INIT to initialize the firmware.
o   If the completion pointer is NIL, then prepares for synchronous 
    communications.  If it is not NIL, prepares for asynchronous printing.
o   Calls AppleTalk PAPopen to make connection, returning an error if one is 
    returned to you.
o   Stores the AppleTalk Session number in the PAPRead, PAPWrite and PAPClose 
    parameter blocks.
o   Executes an RTL if there is no completion routine (pointer is NIL), 
    otherwise perform a JSL to the completion routine.


PrDevRead                $1D13

Description:
    This call reads input from the printer.

Input:                   WORD        space for result
                         LONG        buffer pointer
                         WORD        number of bytes to transfer
 
Output:                  WORD        number of bytes transferred 

Direct Connect:
o   Reads a specified number of bytes from the printer into the buffer.

Network:
o   Calls AppleTalk PAPRead to read synchronously.  Since there is no 
    completion pointer, reading from a network device must always be done 
    synchronously.  To read asynchronously, use PrDevAsyncRead.


PrDevWrite              $1E13

Description:
    Writes the data in the buffer to the printer and calls the completion 
    routine.

Input:                   LONG    write completion pointer
                         LONG    buffer pointer
                         WORD    buffer length

Direct Connect:
o   Writes the contents of the buffer to the printer.
o   If the completion pointer is NIL, then RTL.  If it is not, then perform a 
    JSL to the completion routine.

Network:
o   If the completion pointer is NIL, then writing will occur synchronously.  
    Otherwise, writing will occur asynchronously.
o   Calls AppleTalk PAPWrite to transfer the contents of the buffer.
o   If the completion pointer is NIL, then RTL to the caller.  Otherwise, 
    perform a JSL to the completion routine first.


PrDevClose               $1F13

Description:
    This call is not required to do anything.  However, if you allocate any 
    system resources with PrDevOpen, you should deallocate them at this time.  
    As with start and shutdown, note that PrDevClose could be called without a 
    balancing PrDevOpen (the reverse is not true), and you must be prepared for 
    this if you try to deallocate resources which were never allocated.

Input:                   none

Direct Connect:
o   No required function.

Network:
o   Sets End-Of-Write parameter in AppleTalk PAPWrite parameter block to one.
o   Calls PAPWrite with no data.
o   Calls PAPClose.


PrDevStatus              $2013

Description:
    This call performs differently for direct connect and network drivers.  For 
    direct connect drivers, it currently has no required function, although it 
    may return the status of the port in the future.  For network drivers, it 
    calls an AppleTalk status routine, which returns a status string in the 
    buffer (normally a string like "Status:  The print server is spooling your 
    document").

Input:                   LONG        status buffer pointer

Direct Connect:
o   Does nothing.

Network:
o   Calls AppleTalk PAPStatus.


PrDevAsyncRead          $2113

Description:
    Since PrDevRead cannot read asynchronously, this call is provided for that 
    task.  Note that this does nothing for direct connect drivers, and if the 
    completion pointer is NIL, it behaves for network drivers exactly as 
    PrDevRead does.

Input:                   WORD        space for result
                         LONG        completion pointer
                         WORD        buffer length
                         LONG        buffer pointer

Output:                  WORD        number of bytes transferred

Direct Connect:
o   Does nothing.

Network:
o   If the completion pointer is NIL, then performs exactly as PrDevRead.
o   Calls AppleTalk PAPRead.
o   The actual length read is passed back in the PAPRead parameter block.
o   JSL to the completion routine, which pushes the length read onto the stack


PrDevWriteBackground    $2213

Description:
    This routine is not implemented at this time.

Input:                   LONG        completion procedure pointer
                         WORD        buffer length
                         LONG        buffer pointer


PrPortVer               $2413

Description:
    Returns the version number of the currently installed port driver.

Input:                   WORD        space for result

Output:                  WORD        Port driver's version number

Direct Connect and Network:
o   Gets the internal version number of the port driver and returns it on the 
    stack.

Note:
The internal version number is stored as a major byte and a minor byte 
(i.e., $0103 represents version 1.3)


PrDevIsItSafe            $3013

Description:
    This call checks to see if the port or card which your driver controls is 
    enabled.  It should check at least the corresponding bit of $E0C02D, and 
    checking the Battery RAM settings wouldn't hurt any either.

Input:                   LONG        printer name pointer
Input:                   WORD        space for result

Output:                  WORD        Boolean indicating if port is 
                                     enabled 

Direct Connect and Network:
o   Checks the system to see if the hardware and/or firmware for the card or 
    port this driver controls is enabled, and returns TRUE if it is safe to 
    proceed and FALSE if not.  Note that for a port driver that controls an 
    interface card, this call should return FALSE if the card is disabled and 
    the port is enabled, while for a port driver which controls an Apple IIGS 
    internal port, the returned value should be TRUE if the port is enabled and 
    FALSE if not.


Further Reference
_____________________________________________________________________________
    o    Apple IIGS Toolbox Reference, Volumes 1 & 2
    o    Apple IIGS Technical Note #35, Printer Driver Specifications

