SECTION 09050

BASIC FINISH ACCESSORIES

PART	GENERAL

SECTION INCLUDES

Stucco and plaster accessories.

Gypsum board accessories.

Exterior insulation and finish system (EIFS) accessories.

Direct-applied exterior finish system (DEFS) accessories.

RELATED SECTIONS

Section 07240 - Exterior Insulation and Finish System.

Section 07241 - Direct-Applied Exterior Finish System.

Section 09210 - Gypsum Plaster.

Section 09220 - Portland Cement Plaster.

Section 09260 - Gypsum Board Assemblies.

Section _____ - _______________________________.

REFERENCES

ASTM C 1063 - Installation of Lathing and Furring to Receive Interior and Exterior Portland Cement-Based Plaster.

ASTM D 1784 - Rigid Poly(Vinyl Chloride) (PVC) Compounds and Chlorinated Poly(Vinyl Chloride) (CPVC) Compounds.

PART	PRODUCTS

MANUFACTURERS

Acceptable Manufacturer: Plastic Components, Inc. (PCI), 9051 NW 97th Terrace, Miami, FL 33178; ASD. Tel: (305) 885-0561 or (800) 327-7077; Fax: (305) 887-2452.

Requests for substitutions will be considered in accordance with provisions of Section 01600.

Substitutions: Not permitted.

Provide all basic finish accessories from a single manufacturer.

MATERIALS

Polyvinyl Chloride (PVC): ASTM D 1784, cell classification 13244C.

PORTLAND CEMENT PLASTER (STUCCO) ACCESSORIES

Soffit Vents:

PCI 300, 2-5/8 inches (66.7 mm) vent area, 15 sq. in./lineal foot (31,750 sq mm/m) free air flow.

PCI 301, 1-3/4 inches (44.5 mm) vent area, 7 sq. in./lineal foot (14,817 sq mm/m)free air flow.

PCI 3300, 3 inches (76.2 mm)vent area, 15 sq. in./lineal foot (31,750 sq mm/m)free air flow.

PCI 4300, 4 inches (101.6 mm)vent area, 16 sq. in./lineal foot (33,867 sq mm/m)free air flow.

Continuous Soffit Vents:

PCI 549-50, 1/2 inch (12.7 mm)ground, 2-3/8 inches (60.3 mm) vent area, 15 sq. in./lineal foot (31,750 sq mm/m) free air flow.

PCI 549-58, 5/8 inch (15.8 mm)ground, 2-3/8 inches (60.3 mm) vent area, 15 sq. in./lineal foot (31,750 sq mm/m) free air flow.

PCI 549-75, 3/4 inch (19.1 mm)ground, 2-3/8 inches (60.3 mm) vent area, 15 sq. in./lineal foot (31,750 sq mm/m) free air flow.

PCI 549-78, 7/8 inch (22.2 mm)ground, 2-3/8 inches (60.3 mm) vent area, 15 sq. in./lineal foot (31,750 sq mm/m) free air flow.

"Ultra-Trac" Plaster Reveals:

PCI 707-50, 1/2 inch (13 mm) wide, 1/2 inch (13 mm) ground.

PCI 708-25, 3/4 inch (19 mm) wide, 1/4 inch (6 mm) ground.

PCI 708-38, 3/4 inch (19 mm) wide, 3/8 inch (9.5 mm) ground.

PCI 708-50, 3/4 inch (19 mm) wide, 1/2 inch (13 mm) ground.

PCI 708-58, 3/4 inch (19 mm) wide, 5/8 inch (16 mm) ground.

PCI 708-75, 3/4 inch (19 mm) wide, 3/4 inch (19 mm) ground.

PCI 709-25, 1 inch (25.4 mm) wide, 1/4 inch (6 mm) ground.

PCI 709-38, 1 inch (25.4 mm) wide, 3/8 inch (9.5 mm) ground.

PCI 709-50, 1 inch (25.4 mm) wide, 1/2 inch (13 mm) ground.

PCI 709-58, 1 inch (25.4 mm) wide, 5/8 inch (16 mm) ground.

PCI 709-75, 1 inch (25.4 mm) wide, 3/4 inch (19 mm) ground.

PCI 710-25, 1-1/2 inches (38 mm) wide, 1/4 inch (6 mm) ground.

PCI 710-38, 1-1/2 inches (38 mm) wide, 3/8 inch (9.5 mm) ground.

PCI 710-50, 1-1/2 inches (38 mm) wide, 1/2 inch (13 mm) ground.

PCI 710-58, 1-1/2 inches (38 mm) wide, 5/8 inch (16 mm) ground.

PCI 710-75, 1-1/2 inches (38 mm) wide, 3/4 inch (19 mm) ground.

PCI 711-25, 2 inches (50.8 mm) wide, 1/4 inch (6 mm) ground.

PCI 711-38, 2 inches (50.8 mm) wide, 3/8 inch (9.5 mm) ground.

PCI 711-50, 2 inches (50.8 mm) wide, 1/2 inch (13 mm) ground.

PCI 711-58, 2 inches (50.8 mm) wide, 5/8 inch (16 mm) ground.

PCI 711-75, 2 inches (50.8 mm) wide, 3/4 inch (19 mm) ground.

PCI 712-50, 2-1/2 inches (63.5 mm) wide, 1/2 inch (13 mm) ground.

PCI 712-58, 2-1/2 inches (63.5 mm) wide, 5/8 inch (16 mm) ground.

PCI 712-75, 2-1/2 inches (63.5 mm) wide, 3/4 inch (19 mm) ground.

PCI 713-50, 3 inches (76.2 mm) wide, 1/2 inch (13 mm) ground.

PCI 713-58, 3 inches (76.2 mm) wide, 5/8 inch (16 mm) ground.

PCI 713-75, 3 inches (76.2 mm) wide, 3/4 inch (19 mm) ground.

PCI 714-50, 4 inches (101.6 mm) wide, 1/2 inch (13 mm) ground.

PCI 714-75, 4 inches (101.6 mm) wide, 3/4 inch (19 mm) ground.

"Ultra-Trac" 90-Degree Plaster Reveal Angle Intersections:

PCI PRA-75-25, for 1/4 inch (6 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRA-75-38, for 3/8 inch (9.5 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRA-75-50, for 1/2 inch (13 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRA-75-58, for 5/8 inch (16 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRA-75-75, for 3/4 inch (19 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRA-1-25, for 1/4 inch (6 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRA-1-38, for 3/8 inch (9.5 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRA-1-50, for 1/2 inch (13 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRA-1-58, for 5/8 inch (16 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRA-1-75, for 3/4 inch (19 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRA-15-25, for 1/4 inch (6 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRA-15-38, for 3/8 inch (9.5 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRA-15-50, for 1/2 inch (13 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRA-15-58, for 5/8 inch (16 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRA-15-75, for 3/4 inch (19 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRA-2-38, for 3/8 inch (9.5 mm)ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRA-2-50, for 1/2 inch (13 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRA-2-58, for 5/8 inch (16 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRA-2-75, for 3/4 inch (19 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRA-25-50, for 1/2 inch (13 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRA-25-58, for 5/8 inch (16 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRA-25-75, for 3/4 inch (19 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRA-3-50, for 1/2 inch (13 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRA-3-58, for 5/8 inch (16 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRA-3-75, for 3/4 inch (19 mm) ground 3 inch (76.2 mm) wide plaster reveal.

"Ultra-Trac" Plaster Reveal Cross Intersections:

PCI PRC-75-25, for 1/4 inch (6 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRC-75-38, for 3/8 inch (9.5 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRC-75-50, for 1/2 inch (13 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRC-75-58, for 5/8 inch (16 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRC-75-75, for 3/4 inch (19 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRC-1-25, for 1/4 inch (6 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRC-1-38, for 3/8 inch (9.5 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRC-1-50, for 1/2 inch (13 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRC-1-58, for 5/8 inch (16 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRC-1-75, for 3/4 inch (19 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRC-15-25, for 1/4 inch (6 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRC-15-38, for 3/8 inch (9.5 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRC-15-50, for 1/2 inch (13 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRC-15-58, for 5/8 inch (16 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRC-15-75, for 3/4 inch (19 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRC-2-38, for 1/4 inch (6 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRC-2-50, for 1/2 inch (13 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRC-2-58, for 5/8 inch (16 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRC-2-75, for 3/4 inch (19 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRC-25-50, for 1/2 inch (13 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRC-25-58, for 5/8 inch (16 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRC-25-75, for 3/4 inch (19 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRC-3-50, for 1/4 inch (6 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRC-3-58, for 5/8 inch (16 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRC-3-75, for 3/4 inch (19 mm) ground 3 inch (76.2 mm) wide plaster reveal.

"Ultra-Trac" Plaster Reveal End Stops:

PCI PRES-75-25, for 1/4 inch (6 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRES-75-38, for 3/8 inch (9.5 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRES-75-50, for 1/2 inch (13 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRES-75-58, for 5/8 inch (16 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRES-75-75, for 3/4 inch (19 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRES-1-25, for 1/4 inch (6 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRES-1-38, for 3/8 inch (9.5 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRES-1-50, for 1/2 inch (13 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRES-1-58, for 5/8 inch (16 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRES-1-75, for 3/4 inch (19 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRES-15-25, for 1/4 inch (6 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRES-15-38, for 3/8 inch (9.5 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRES-15-50, for 1/2 inch (13 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRES-15-58, for 5/8 inch (16 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRES-15-75, for 3/4 inch (19 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRES-2-38, for 3/8 inch (9.5 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRES-2-50, for 1/2 inch (13 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRES-2-58, for 5/8 inch (16 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRES-2-75, for 3/4 inch (19 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRES-25-50, for 1/2 inch (13 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRES-25-58, for 5/8 inch (16 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRES-25-75, for 3/4 inch (19 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRES-3-50, for 1/2 inch (13 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRES-3-58, for 5/8 inch (16 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRES-3-75, for 3/4 inch (19 mm) ground 3 inch (76.2 mm) wide plaster reveal.

"Ultra-Trac" Plaster Reveal Inside Corners:

PCI PRIC-75-25, for 1/4 inch (6 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRIC-75-38, for 3/8 inch (9.5 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRIC-75-50, for 1/2 inch (13 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRIC-75-58, for 5/8 inch (16 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRIC-75-75, for 3/4 inch (19 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRIC-1-25, for 1/4 inch (6 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRIC-1-38, for 3/8 inch (9.5 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRIC-1-50, for 1/2 inch (13 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRIC-1-58, for 5/8 inch (16 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRIC-1-75, for 3/4 inch (19 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRIC-15-25, for 1/4 inch (6 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRIC-15-38, for 3/8 inch (9.5 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRIC-15-50, for 1/2 inch (13 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRIC-15-58, for 5/8 inch (16 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRIC-15-75, for 3/4 inch (19 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRIC-2-38, for 3/8 inch (9.5 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRIC-2-50, for 1/2 inch (13 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRIC-2-58, for 5/8 inch (16 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRIC-2-75, for 3/4 inch (19 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRIC-25-50, for 1/2 inch (13 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRIC-25-58, for 5/8 inch (16 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRIC-25-75, for 3/4 inch (19 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRIC-3-50, for 1/2 inch (13 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRIC-3-58, for 5/8 inch (16 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRIC-3-75, for 3/4 inch (19 mm) ground 3 inch (76.2 mm) wide plaster reveal.

"Ultra-Trac" Plaster Reveal Outside Corners:

PCI PROC-75-25, for 1/4 inch (6 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PROC-75-38, for 3/8 inch (9.5 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PROC-75-50, for 1/2 inch (13 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PROC-75-58, for 5/8 inch (16 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PROC-75-75, for 3/4 inch (19 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PROC-1-25, for 1/4 inch (6 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PROC-1-38, for 3/8 inch (9.5 mm)ground 1 inch (25.4 mm) wide plaster reveal.

PCI PROC-1-50, for 1/2 inch (13 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PROC-1-58, for 5/8 inch (16 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PROC-1-75, for 3/4 inch (19 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PROC-15-25, for 1/4 inch (6 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PROC-15-38, for 3/8 inch (9.5 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PROC-15-50, for 1/2 inch (13 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PROC-15-58, for 5/8 inch (16 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PROC-15-75, for 3/4 inch (19 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PROC-2-38, for 3/8 inch (9.5 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PROC-2-50, for 1/2 inch (13 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PROC-2-58, for 5/8 inch (16 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PROC-2-75, for 3/4 inch (19 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PROC-25-50, for 1/2 inch (13 mm) ground 2-1/2 inch wide plaster reveal.

PCI PROC-25-58, for 5/8 inch (16 mm) ground 2-1/2 inch wide plaster reveal.

PCI PROC-25-75, for 3/4 inch (19 mm) ground 2-1/2 inch wide plaster reveal.

PCI PROC-3-50, for 1/2 inch (13 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PROC-3-58, for 5/8 inch (16 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PROC-3-75, for 3/4 inch (19 mm) ground 3 inch (76.2 mm) wide plaster reveal.

"Ultra-Trac" Plaster Reveal T-Intersections:

PCI PRT-75-25, for 1/4 inch (6 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRT-75-38, for 3/8 inch (9.5 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRT-75-50, for 1/2 inch (13 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRT-75-58, for 5/8 inch (16 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRT-75-75, for 3/4 inch (19 mm) ground 3/4 inch (19 mm) wide plaster reveal.

PCI PRT-1-25, for 1/4 inch (6 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRT-1-38, for 3/8 inch (9.5 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRT-1-50, for 1/2 inch (13 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRT-1-58, for 5/8 inch (16 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRT-1-75, for 3/4 inch (19 mm) ground 1 inch (25.4 mm) wide plaster reveal.

PCI PRT 15-25, for 1/4 inch (6 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRT-15-38, for 3/8 inch (9.5 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRT-15-50, for 1/2 inch (13 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRT-15-58, for 5/8 inch (16 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRT-15-75, for 3/4 inch (19 mm) ground 1-1/2 inch (38 mm) wide plaster reveal.

PCI PRT-2-38, for 3/8 inch (9.5 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRT-2-50, for 1/2 inch (13 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRT-2-58, for 5/8 inch (16 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRT-2-75, for 3/4 inch (19 mm) ground 2 inch (50.8 mm) wide plaster reveal.

PCI PRT-25-50, for 1/2 inch (13 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRT-25-58, for 5/8 inch (16 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRT-25-75, for 3/4 inch (19 mm) ground 2-1/2 inch (63.5 mm) wide plaster reveal.

PCI PRT-3-50, for 1/2 inch (13 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRT-3-58, for 5/8 inch (16 mm) ground 3 inch (76.2 mm) wide plaster reveal.

PCI PRT-3-75, for 3/4 inch (19 mm) ground 3 inch (76.2 mm) wide plaster reveal.

"T" Bar Casing Beads:

PCI 1100, 1 inch (25.4 mm) ground, 1-3/4 inch (44.5 mm) wide perforated flange.

PCI 1125, 1-1/4 inch (31.8 mm) ground, 1-3/4 inch (44.5 mm) wide perforated flange.

PCI 1150, 1-1/2 inch (38 mm) ground, 1-3/4 inch (44.5 mm) wide perforated flange.

PCI 1200, 2 inch (50.8 mm) ground, 1-3/4 inch (44.5 mm) wide perforated flange.

Slip Joints:

PCI 2079, 3/8 inch (9.5 mm) ground, flanges adjustable from 0 to 5/8 inch (16 mm).

PCI 2080, 1/2 inch (13 mm) ground, flanges adjustable from 0 to 5/8 inch (16 mm).

PCI 2081, 3/4 inch (19 mm) ground, flanges adjustable from 0 to 5/8 inch (16 mm).

PCI 2082, 7/8 inch (22.2 mm) ground, flanges adjustable from 0 to 5/8 inch (16 mm).

"Ultra-Lath": PCI PDM2796, rust-proof, self-furring, standard 27 inch by 96 inch (0.686 by 2.438 m) sheets. Also available in 27 inch wide by 100 foot (0.686 by 30.480 m) rolls.

GYPSUM BOARD ACCESSORIES

Continuous Soffit Vents:

PCI 548-38, 2-5/8 inch (66.7 mm) wide vented area, 14 square inches of free air flow per linear foot (296.3 sq cm/m).

PCI 548-50, 2-5/8 inch (66.7 mm) wide vented area, 14 square inches of free air flow per linear foot (296.3 sq cm/m).

PCI 548-58, 2-5/8 inch (66.7 mm) wide vented area, 14 square inches of free air flow per linear foot (296.3 sq cm/m).

PCI 548-75, 2-5/8 inch (66.7 mm)} wide vented area, 14 square inches of free air flow per linear foot (296.3 sq cm/m).

PCI 3548-50, 3 inch (76.2 mm) wide vented area, 15 square inches of free air flow per linear foot (317.5 sq cm/m).

PCI 3548-58, 3 inch (76.2 mm) wide vented area, 15 square inches of free air flow per linear foot (317.5 sq cm/m).

PCI 4548-50, 4 inch (101.6 mm) wide vented area, 16 square inches of free air flow per linear foot (338.7 sq cm/m).

PCI 4548-58, 4 inch (101.6 mm) wide vented area, 16 square inches of free air flow per linear foot (338.7 sq cm/m).

Drywall Reveals:

PCI 225, 1/2 inch (13 mm) reveal.

PCI 226, 1 inch (25.4 mm) reveal.

PCI 227, 3/4 inch (19 mm) reveal.

PCI 228, 3/8 inch (9.5 mm) reveal.

PCI 229, 5/8 inch (16 mm) reveal.

PCI 235, 1-1/2 inch (38 mm) reveal.

PCI 236, 2 inch (50.8 mm) reveal.

PCI 237, 3 inch (76.2 mm) reveal.

EXTERIOR INSULATED FINISH SYSTEM (EIFS) ACCESSORIES

STARTER TRAC(R):

PCI ST-50.

PCI ST-58.

PCI ST-75.

PCI ST-1.

PCI ST-1.25.

PCI ST-15.

PCI ST-1.75.

PCI ST-2.

PCI ST-2.25.

PCI ST-25.

PCI ST-2.75.

PCI ST-3.

PCI ST-35.

PCI ST-4.

STARTER TRAC(R) Drip Edge:

PCI STDE-50.

PCI STDE-58.

PCI STDE-75.

PCI STDE-1.

PCI STDE-1.25.

PCI STDE-15.

PCI STDE-1.75.

PCI STDE-2.

PCI STDE-2.25.

PCI STDE-25.

PCI STDE-2.75.

PCI STDE-3.

PCI STDE-35.

PCI STDE-4.

Soffit Vent: PCI 548-1.

DIRECT-APPLIED EXTERIOR FINISH SYSTEM (DEFS) ACCESSORIES

Bullnose Veneer Bead:

PCI 208HI, 1 inch (25.4 mm) perforated flanges, 3/4 inch (19 mm) radius.

PCI 208HIA, 1 inch (25.4 mm) perforated flanges, one leg slotted.

Control Joint: PCI PLO93.

Soffit Drip Screed:

PCI 2254-50, 1/2 inch (13 mm) reveal, for 1/2 inch (13 mm) sheathing.

PCI 2254-58, 1/2 inch (13 mm) reveal, for 5/8 inch (16 mm) sheathing.

Surface Mounted "J" Bead:

PCI 2201-50.

PCI 2201-58.

Corner Bead: PCI 2209, 1-1/2 inch by 1-1/2 inch (38 by 38 mm) flange and grooved.

Surface Mounted "L" Bead:

PCI 2221-50.

PCI 2221-58.

PCI 2221-1.

PART	EXECUTION

INSTALLATION

Install accessories in accordance with accepted industry standards, applicable codes, and manufacturer's recommendations.

Staple, nail, screw, or glue gypsum board accessories into place in accordance with ASTM C 1063.

Install EIFS/DEFS accessories in accordance with recommendations of system manufacturer.

Caulk all butt joints, intersections, and ends.

END OF SECTION