Solid wheels like this were made from a section of a tree-trunk, which were rounded off appropriately. They were not very tough and soon broke apart. The first advances were fixed axles on which the wheel turned. It was secured with wooden pins on the axle.