First-class levers like this act as a seesaw. The load and effort can be exerted on either side of the fulcrum.