On a motorcycle the engine power is transmitted to the rear wheel by means of either a chain or a transaxle with a drive shaft. A chain must be frequently tightened, while a transaxle is almost maintenance-free.