; Packet TNC inizialization file
; Place only packet commands in this file
; Each line must be CR/LF terminated.
; Comment and space lines are permitted. Comment lines must begin
; with a semi-colon in the first column and space lines must consist
; of a CR/LF sequence only.

; The contents of this file is automatically sent to the respecitve TNC
; whenever you first activate a packet port. A RESET command will not send
; this file!

; If you have multiple Packet TNCs make sure you provide one file for 
; each port. The file must be named XXXXXXXX.INS, where XXXXXXXX is the 
; port name (same as the Packet configuration file name). The extension 
; must be INS.


ECHO OFF
FLOW OFF
NEWMODE ON
NOMODE OFF
BBSMSGS ON
XFLOW OFF
XON $00
XOFF $00
START $00
STOP $00
MONITOR OFF
MYCALL xxxxxx  <-- place your call sign here
AWLEN 8
8BIT ON
