### Assemble and link the EtherTalk ROM.
asm -l  EtherROM.a

Link EtherROM.a.o     -o EtherROM

### Patch the crc value and convert the code to a data file, to
### make it a file that can be downloaded to a ROM burner.
"{Decl}Decl.Tools:crcPatch"  EtherROM
"{Decl}Decl.Tools:Data"  EtherROM  EtherROM.d
