{[j=15-/40]}
{$R-}
PROGRAM NuBusTest;
{ This program determines whether or not this machine can deal with NuBus cards
 that put their declaration ROM in the high part of the cardŐs 16M address
 space. Specifically, it checks to see if the machine is running ROM 78, and if
 so, whether or not the rom version is later than 1.0 (i.e. has a DeclROM) }

	USES
			Memtypes, Quickdraw, OSIntf, ToolIntf, PackIntf, nbTestIntf;

	PROCEDURE _DataInit;
		EXTERNAL;

	BEGIN
		UnLoadSeg(@_DataInit);
		InitGraf(@thePort);
		InitFonts;
		FlushEvents(everyEvent, 0);
		InitWindows;
		InitMenus;
		TEInit;
		InitDialogs(NIL);
		InitCursor;

		IF CheckNuBus THEN {Nothing} ;
	END.
