Installation

Equipment required

-
A Macintosh® personal computer running system 7.x, with a hard disk.
- 1 megabyte of available RAM*.
-
A modem (Hayes™ or Hayes-compatible)
-
A standard telephone line

* This is the application needed RAM partition.

Installing the software

The folder called hi-BBS™ User ƒ containing this guide also contains the hi-BBS Client application in a folder called hi-BBS™ Client ƒ. Another folder called Put these in System ƒ contains the files needed by the hi-BBS Client to connect to the hi-BBS Server. A description of these CTB Tools is given below: 

AppleTalk ADSP Tool: 
This Connection Tool is used to connect with the hi-BBS server over AppleTalk.

Apple Modem Tool: 
This Connection Tool is used to connect with the hi-BBS server using a modem.

XModem Tool:
This is the File Transfer Tool used to exchange documents with the server.

These files are the only things needed to install hi-BBS on your computer.

• Drag these files over the System folder on your hard disk, then release to copy them to the proper location (Extensions folder).

You are now ready to go on-line.